**Dimmer Dynamic Arch**

|  |  |  |  |
| --- | --- | --- | --- |
| **Task** | **Periodicity**  **(ms)** | **Priority** | **First Delay(Ticks)** |
| AppInit\_tasl | 5 | 0 | 0 |
| Com\_task | 5 | 1 | 20 |
| Switch\_task | 5 | 2 | 20 |
| Rte\_task | 40 | 3 | 20 |

**Tick Time = 5 mSec**